1. SRS components are located in this area. Review the SRS component locations LHD, SRS component locations RHD and the precautions and procedures before performing repairs or service. NOTE: Put on gloves to protect your hands. Take care not to scratch the body and related parts. Remove these items from the left side of the vehicle: Front door sill trim Rear door sill trim Center pillar lower trim
   - | Without side curtain airbag
   - | With side curtain airbag
   Rear seat cushion Trunk lid trim Trunk rear trim panel
   - | Without trunk side spacer
   - | With trunk side spacer
   Trunk side trim panel, left side
   - | Without trunk side spacer
   - | With trunk side spacer
Trunk lid hinge cover Pull the carpet back as needed. Disconnect the trunk lid opener/fuel fill door opener cable (A) from the opener (B) LHD: Release the opener cable from the clip (C). Remove the cushion tape (E). RHD: Release the opener cable from the clips (C, D). Remove the cushion tape (E). | LHD RHD