M/T Change Lever Clearance Inspection

1. Measure the clearance between change lever (A) and the select lever (B) with a feeler gauge (C). If the clearance is more than the service limit, go to Step 2 .
   Standard: | 0.05−0.25 mm (0.002−0.010 in.)
   Service Limit: | 0.5 mm (0.020 in.)

1. Measure the groove of the change lever. If distance is not within the standard, replace the change lever with a new one. If distance is within the standard, replace the select lever with a new one.
   Standard: | 15.00−15.10 mm (0.591−0.594 in.)