Special Tool Required Driver attachment, 42 mm I.D. 07QAD-P0A0100 Install the thrust needle bearing (A), needle bearing (B), 1st gear (C), thrust needle bearing (D), 40 x 51.5 mm thrust washer (E), 1st/3rd clutch (F), and 3rd gear collar (G) on the secondary shaft (H). Install the idler gear (I), then install the ball bearing (J) on the idler gear with the special tool and a press. Install the conical spring washer (K) and locknut (L), then tighten the locknut to 29 N·m (3.0 kgf·m, 22 lbf·ft). |