Power Mirror Actuator Test

Remove the door panel. Disconnect the 13P connector (A) from the power mirror actuator (B). |

Check actuator operation by connecting power and ground according to the table. If the mirror fails to work properly, replace the mirror actuator. |

Defogger Test Check for continuity between the No. 2 and No. 7 terminals of the 13P connector. There should be continuity with the defogger switch ON. If there is no continuity, check for an open circuit. |