ABS indicator does not come on Turn the ignition switch ON (II), and watch the ABS indicator. Does the ABS indicator come on for several seconds?
YES | - | The system is OK at this time.■
NO | - | Go to Step 2 .
Do the gauge control module self-diagnosis function procedure. Is gauge control module OK?
YES | - | Go to Step 3 .
NO | - | Replace gauge control module. ■
Turn the ignition switch OFF. Remove the gauge control module. Disconnect the gauge control module connector B (30P). Check for continuity between gauge control module connector B (30P) terminal No. 27 and the body ground. Is there continuity?
YES | - | Repair short to body ground in the wire between the gauge control module and the ABS modulator-control unit.■
NO | - | Check for loose terminals in the gauge control module connectors. If connectors are OK, replace the gauge control module.■