Reverse shift lever

Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
Reverse shift lever | Finger thickness |  | 6.400−6.650 mm (0.2520−0.2618 in.) | ———
Shift lever-to-shift fork clearance |  | 0.05−0.50 mm (0.002−0.020 in.) | 0.6 mm (0.024 in.)
Shift lever diameter at contact area |  | 13.0−13.2 mm (0.51−0.52 in.) | ———
Shift lever-to-interlock clearance |  | 0−0.4 mm (0−0.015 in.) | 0.5 mm (0.020 in.)