Special Tools Required Engine sub hanger plate 07MAK-PY30100 Remove all of the old liquid gasket from the oil pan mating surfaces, bolts, and bolt holes. Clean and dry the oil pan mating surfaces. Apply liquid gasket, P/N 08C70-K0334M or 08C70-X0331S, evenly to the engine block mating surface of the oil pan and to the inner threads of the bolt holes. NOTE: Do not install the parts if 4 minutes or more have elapsed since applying liquid gasket. Instead, reapply liquid gasket after removing old residue. Install the oil pan. |