Measure voltage between PGM-FI main relay 2 (FUEL PUMP) 4P connector terminal No. 1 and body ground. Is there battery voltage?
YES | - | Replace the inertia switch .■
NO | - | Replace the No.19 FUEL PUMP (15 A) fuse in the under-dash fuse/relay box.■ If needed, replace the under-dash fuse/relay box.■ If needed, repair open in wires between inertia switch and under-dash fuse/relay box.■
Turn the ignition switch OFF. |