Camshaft/Rocker Arm, Camshaft Seal, and Pulley Installation

Reassemble the rocker arm assembly. Clean and dry the No. 5 rocker shaft holder mating surface. Apply liquid gasket, P/N 08C70-K0234M, 08C70-K0334M, or 08C70-X0331S, evenly to the cylinder head mating surface of the No. 5 rocker shaft holder. NOTE: Do not install the parts if 4 minutes or more have elapsed since applying liquid gasket. Instead, reapply liquid gasket after removing old residue. |

Insert the bolts (A) into the rocker shaft holder, then install the rocker arm assembly (B) on the cylinder head. Remove the bolts from the rocker shaft holder. |

Make sure the punch marks on the variable valve timing control (VTC) actuator and exhaust camshaft sprocket are facing up, then set the camshafts (A) in the holder. Set the camshaft holders (B) and cam chain guide B (C) in place. |

1. Tighten the bolts to the specified torque.
   Specified Torque
   8 mm Bolts: | 22 N·m (2.2 kgf·m, 16 lbf·ft)
   6 mm Bolts: | 12 N·m (1.2 kgf·m, 8.7 lbf·ft)
   6 mm Bolts: | (21), (22), (23)
Install the cam chain, and adjust the valve clearance. |