Engine Mount Bracket Removal/Installation - Side

Support the engine with a jack and wood block under the oil pan. Remove the ground cable (A), then remove the upper torque rod (B). |

Remove the side engine mount bracket (A). Install the side engine mount bracket, then loosely tighten the new bolts/nut (B), and loosely tighten the bolt (C). Remove the air cleaner housing. |

Loosen the transmission upper mount bracket bolt (A) and transmission upper mount bolt/nuts (B). Remove a jack. |

Tighten the side engine mount mounting bolts/nut in the numbered sequence shown. |

Tighten the transmission upper mount/bracket mounting bolts/nuts in the numbered sequence shown. |

Install the upper torque rod (A), then tighten the new bolts in the numbered sequence shown. Install the ground cable (B). Install the air cleaner housing. |