Reassembly Apply Molykote 44MA or Solvest 842M grease to the sliding surface of the pivot pin (A), and insert the pin into the brake shoe (B) for the rear side. Install the parking brake lever (C) and wave washer (D) on the pivot pin, and secure with a new U-clip (E). Install the wave washer with its convex side facing out. Pinch the U-clip securely to prevent the pivot pin from coming out from the brake shoe. |