M/T Clutch Housing Countershaft Bearing Replacement

Special Tools Required Adjustable bearing puller, 45−75 mm 07YAC-0010100 Attachment, 72 x 75 mm 07746-0010600 Driver 07749-0010000 Bearing remover shaft 07JAC-PH80200 Slide hammer 07741-0010201 Remove the bearing set plate (A) from the clutch housing (B). |

Remove the needle bearing (A) from the clutch houshing (B) using the special tools. |

Install the new needle bearing (A) using the special tools. |

Install the bearing set plate (A) with bolts (B). |