Maintenance Schedule for Severe Conditions
25,000miles(2year)

Follow the Severe Conditions Maintenance Schedule if the customer's vehicle is driven MAINLY under one or more of the following conditions:

- Driving less than 8 km (5 miles) per trip or, in freezing temperatures, driving less than 16 km (10 miles) per trip.
- Driving in extremely hot over 35 °C (95 °F) conditions.
- Extensive idling, or long periods of stop-and-go-driving.
- Trailer towing, driving with a car-top carrier, or driving in mountainous conditions.
- Driving on muddy, dusty, or de-iced roads.

NOTE: If the customer's vehicle is driven OCCASIONALLY under severe conditions, follow the Normal Conditions Maintenance Schedule.

Service at the indicated distance or time whichever comes first

| Replace engine oil filter

| Check parking brake adjustment

| Check lights alignment
Check the position of the headlights

| Test drive
Check for road stability, noise, vibration, and dashboard operation

| Check expiry date for IMS bottle (if equipped)

| Inspect drive belts
Check for cracks, damage, deflection, and tension

| Replace dust and pollen filter
When the customer drives primarily in urban areas that have high concentrations of soot in the air, under dusty conditions, or the air flow from the heating and cooling system/climate control system becomes less than normal.

Visually inspect the following items:
|  | Check for correct installation and position, check for cracks, deterioration, rust, and leaks
|  | Check tightness of screws, nuts, and joints. If necessary, retighten

| Brake hoses and lines (including ABS/VSA)
Check the master cylinder, proportioning control valve, and ABS/VSA modulator control-unit and leakage

| All fluid levels and condition of fluids
Check levels and check for leaks. If necessary, add engine coolant , MTF, ATF, brake fluid, power steering fluid , and windshield fluid

| Exhaust system
Check the exhaust pipe and muffler for damage, leaks, and tightness

| Fuel lines and connections
Check fuel lines for loose connections, cracks and deterioration. Retighten loose connections and replace any damaged parts

| Tyre condition
Check for pressure, puncture, cuts, and irregular thread wear

Every 10,000 km (6,250 miles) or 6 months

| Replace engine oil

| Inspect front and rear brakes
|  | Check the brake pad and disc thickness. Check for damage or cracks front pad , front disc , rear pad , rear disc
|  | Check the brake linings for cracking, grazing, wear, and contamination
|  | Check the calipers for damage, leaks, and tightness

Every 40,000 km (25,000 miles)

| Replace air cleaner element
Dry type

| Replace spark plugs
K20Z2 engine

| Inspect the valve clearance

Every 20,000 km (12,500 miles)

| Replace air cleaner element
Wet type

| Clean air cleaner element
Dry type only

Every 120,000 km (75,000 miles)

| Replace spark plugs
K24A3 engine

Every 60,000 km (37,500 miles) or 4 years

| Replace manual transmission fluid (MTF)
Use genuine Honda Manual Transmission Fluid (MTF)

At 60,000 km (37,500 miles) or 4 years, then every 40,000 km (25,000 miles) or 2 years

| Replace automatic transmission fluid (ATF)
Use genuine Honda ATF-Z1

At 200,000 km (120,000 miles) or 10 years, then every 100,000 km (60,000 miles) or 5 years

| Replace engine Coolant
Use genuine Honda Long Life Antifreeze/Coolant Type 2

Every 3 years

| Replace brake fluid
Use only DOT 3 or DOT 4 brake fluid. We recommend genuine Honda Brake Fluid. Check that brake fluid level between the upper and lower marks on the reservoir

Every years

| Inspect vehicle corrosion
Paintowork and body work.

Inspect every 10,000 km (6,250 miles) or 6 months

Visually inspect the following items:

| Tie-rod ends, steering gearbox, and boots
Check rack grease and steering linkage. Check the boot for damage and leaking grease

| Suspension components
|  | Check the bolts for tightness
|  | Check all dust cover for deterioration and damage

| Driveshaft boots
|  | Check the boot and boot band for cracks
|  | Check rack grease