Exploded View 5-speed model: 6-speed model: Special Tools Required Driver, 40 mm I.D. 07746-0030100 Attachment, 30 mm I.D. 07746-0030300 NOTE: Refer to the Exploded View as needed during this procedure. 6-speed model is shown, 5-speed model is similar. Clean all parts in solvent, dry them, and apply lubricant to all contact surfaces. Install the distance collar and needle bearing onto the countershaft. Install the triple cone synchro assembly (A) by aligning the synchro cone fingers (B) with 1st gear grooves (C), then install the synchro spring (D). |