M/T Mainshaft Disassembly

Support the ball bearing on the steel blocks, and press the mainshaft out of the ball bearing. |

Support the 5th gear (A) on the steel blocks, and press the mainshaft out of the 5th synchro hub (B). Use of a jaw-type puller can damage the gear teeth. |

Support the 3rd gear (A) on the steel blocks, and press the mainshaft out of the 3rd/4th synchro hub (B). Use of a jaw-type puller can damage the gear teeth. |

Support the angular ball bearing on the steel blocks, and press out the mainshaft. |