VSA OFF Switch Test

Remove the VSA OFF switch (A) from the switch panel. Disconnect the VSA OFF switch 5P connector. |

Check for continuity between the VSA OFF switch 5P connector terminal No. 1 and No. 2. There should be continuity when the switch is pressed, and no continuity when the switch is released. |

Check for continuity between the VSA OFF switch 5P connector terminal No. 3 and No. 4. There should be continuity at all times. |