Disconnect the back-up light switch connector (A). Check for continuity between the No. 1 and No. 2 terminals of the back-up light switch 2P connector. There should be continuity when the shift lever is in reverse. If necessary, replace the back-up light switch . Apply liquid gasket (P/N 08C70-K0234M) to the switch threads, and install the switch on the transmission housing. Tighten the back-up light switch to the specified torque. Install the resonator chamber. Install the battery base, then install the ground cable. Install the air cleaner housing. Install the battery. Connect the positive (+) cable first, then the negative (−) cable to the battery. Enter the anti-theft codes for the radio and navigation system, then enter the customer's radio station presets. Do the power window control unit reset procedure. |