Check for continuity between IMRC valve position sensor 3P connector terminal No. 2 and body ground. Is there continuity?
YES | - | Repair short in the wire between the IMRC valve position sensor and ECM connector No. 1 terminal No. 16, then go to Step 17 .
NO | - | Go to Step 22 .
Turn the ignition switch OFF. Replace the IMRC valve assembly. Reconnect all connectors. Turn the ignition switch ON (II). Reset the ECM with the HDS. Start the engine. Hold the engine speed at 2,000 rpm (min −1 ) without load (in neutral) until the radiator fan comes on, then let it idle. Check for Temporary DTCs or DTCs with the HDS. Are any Temporary DTCs or DTCs indicated?
YES | - | If DTC P2016 is indicated, check for poor connections or loose terminals at the IMRC valve position sensor and the ECM, then go to Step 1 . If any other Temporary DTCs or DTCs are indicated, go to the indicated DTC's troubleshooting.
NO | - | Troubleshooting is complete.■
Update the ECM if it does not have the latest software, or substitute a known-good ECM. Start the engine. Hold the engine speed at 2,000 rpm (min −1 ) without load (in neutral) until the radiator fan comes on, then let it idle. Check for Temporary DTCs or DTCs with the HDS. Are any Temporary DTCs or DTCs indicated?
YES | - | If DTC P2016 is indicated, check for poor connections or loose terminals at the IMRC valve position sensor and the ECM, then go to Step 1 . If any other Temporary DTCs or DTCs are indicated, go to the indicated DTC's troubleshooting.
NO | - | If the ECM was updated, troubleshooting is complete. If the ECM was substituted, replace the original ECM. ■