Special Tools Required A/T oil pressure gauge set 07406-0020004 Before testing, be sure the transmission fluid is filled to the proper level. Lift the vehicle up on a lift or apply the parking brake, block rear wheels, and raise the front of the vehicle. Make sure it is securely supported. Allow the front wheels to rotate freely. Remove the splash shield. Warm up the engine (the radiator fan comes on), then stop it and connect the HDS to the DLC. Connect the oil pressure gauges to the line pressure inspection hole (A) and 4th clutch pressure inspection hole (B). Do not allow dust or other foreign particles to enter the holes while connecting the gauges. |