Remove the drain plug (A), and drain the automatic transmission fluid (ATF). Then reinstall the drain plug with a new sealing washer (B). Disconnect the battery negative terminal, then disconnect the battery positive terminal. Remove the battery hold-down bracket, then remove the battery cover, battery, and battery tray. Remove the intake air duct and air cleaner housing. Loosen the two bolts securing the battery base from under the vehicle, and remove the two bolts securing the battery base in the engine compartment, then remove the battery base. |