DTC 91-2x (91-20 to 91-29, 91-2A to 91-2F): Short in SRS Indicator Erase the DTC memory. Turn the ignition switch ON (II), and check that the SRS indicator comes on for about 6 seconds and then goes off. Does the SRS indicator stay on and is DTC 91-2x indicated?
YES | - | Replace the SRS unit. ■
NO | - | Intermittent failure, system is OK at this time. Go to Troubleshooting Intermittent Failures. If another DTC is indicated, go to the DTC troubleshooting index for troubleshooting details.
Turn the ignition switch OFF. Disconnect the battery negative cable, and wait for 3 minutes. Disconnect SRS unit connector A (28P) from the SRS unit. |