Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
Shift arm | I.D. |  | 15.973−16.005 mm (0.6289−0.6301 in.) | ———
Shift piece diameter at contact area |  | 13.9−14.0 mm (0.54−0.55 in.) | ———
Shift arm-to-shift piece clearance |  | 0.05−0.25 mm (0.002−0.010 in.) | 0.5 mm (0.020 in.)
Select arm | I.D. |  | 11.01−11.05 mm (0.433−0.435 in.) | ———
Interlock diameter at contact area |  | 12.9−13.0 mm (0.50−0.51 in.) | ———
Select arm-to-interlock clearance |  | 0.05−0.25 mm (0.002−0.010 in.) | 0.5 mm (0.020 in.)
Oil pump | Oil pump thrust clearance |  | 0.03−0.13 mm (0.001−0.005 in.) | 0.15 mm (0.006 in.)
Outer rotor-to-body clearance |  | 0.1−0.2 mm (0.004−0.008 in.) | 0.22 mm (0.009 in.)
Inner rotor-to-outer rotor clearance |  | 0.14 mm (0.006 in.) | 0.2 mm (0.008 in.)
Oil pump inner rotor I.D. |  | 17.1−17.2 mm (0.67−0.68 in.) | ———
Oil pump shaft O.D. |  | 16.8−17.0 mm (0.66−0.67 in.) | ———
M/T differential carrier | Backlash |  | 0.4−1.3 mm (0.016−0.051 in.) | ———
Driveshaft contact area I.D. |  | 30.025−30.045 mm (1.1821−1.1829 in.) | ———
Carrier bearing starting torque(preload) |  | 3.43−4.51 N·m (35−46 kgf·cm, 30−40 lbf·in.) | Adjust

Steering

Item | Measurement | Qualification | Standard or New
--- | --- | --- | ---
Steering wheel | Rotational play measured at outside edge with engine running |  | 0−10 mm (0−0.39 in.)
Starting load measured at outside edge with engine running |  | 29 N (3.0 kgf, 6.6 lbf)
Gearbox | Angle of rack guide screw loosened from locked position |  | 10 °−20 °
Pump | Output pressure with shut-off valve closed |  | 8,150−8,850 kPa (83−90 kgf/cm 2 , 1,180−1,280 psi)
Power steering fluid | Capacity Use genuine Honda Power Steering Fluid | Reservoir capacity | 0.4 L (0.42 US qt, 0.36 Imp qt)
System overhaul | 1.1 L (1.16 US qt, 0.97 Imp qt)

Suspension

Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
Wheel alignment | Camber | Front | 0 ° 00 ′±45 ′
Rear | −1 ° 00 ′±30 ′
Caster | Front | 3 ° 12 ′±45 ′
Total toe-in | Front | 0±2 mm (0±0.08 in.)
Rear | 2±2 mm (0.08±0.08 in.)
Front wheel turning angle | Inward | 38 ° 50 ′±2 °
Outward | 31 ° 40 ′ (Reference)
Wheel | Aluminum wheel runout | Axial | 0−0.7 mm (0−0.03 in.) | 2.0 mm (0.08 in.)
Radial | 0−0.7 mm (0−0.03 in.) | 1.5 mm (0.06 in.)
Steel wheel runout | Axial | 0−1.0 mm (0−0.04 in.) | 2.0 mm (0.08 in.)
Radial | 0−1.0 mm (0−0.04 in.) | 1.5 mm (0.06 in.)
Wheel bearing | End play | Front | 0−0.05 mm (0−0.002 in.)
Rear | 0−0.05 mm (0−0.002 in.)

Brakes

Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
Parking brake lever | Distance traveled when lever pulled with 196 N (20 kgf, 44 lbf) of force |  | 8 to 10 clicks
Brake pedal | Pedal height (carpet removed) | LHD type | 144 mm (5.67 in.)
RHD type | 134 mm (5.28 in.)
Free play |  | 1.0−5.0 mm (0.04−0.20 in.)
Master cylinder | Piston-to-pushrod clearance |  | No adjust
Brake disc | Thickness | Front | 24.9−25.1 mm (0.98−0.99 in.) | 23.0 mm (0.91 in.)
Rear | 9.9−10.1 mm (0.39−0.40 in.) | 8.0 mm (0.31 in.)
Runout | Front | ——— | 0.10 mm (0.004 in.)
Rear | ——— | 0.10 mm (0.004 in.)
Parallelism | Front and rear | ——— | 0.015 mm (0.0006 in.)
Brake pad | Thickness | Front | 10.5−11.5 mm (0.41−0.45 in.) | 1.6 mm (0.06 in.)
Rear | 8.9−9.1 mm (0.350−0.358 in.) | 1.6 mm (0.06 in.)
Parking brake shoe | Lining thickness |  | 3.2 mm (0.13 in.) | 1.0 mm (0.04 in.)
Parking brake drum | I.D. |  | 170 mm (6.69 in.) | 171 mm (6.73 in.)
Brake booster | Master cylinder oil pressure | Vacuum kPa (mmHg, in.Hg) | Brake pedal force N (kgf, lbf) | Oil pressure kPa (kgf/cm 2 , psi)
0 (0, 0) | 98 (10, 22) | 0 (0, 0)
294 (30, 66) | 545 (5.6, 80)
66.7 (500, 19.7) | 98 (10, 22) | 5,015 (51.1, 727)
294 (30, 66) | 9,570 (97.6, 1,388)

Air Conditioning

Item | Measurement | Qualification | Standard or New
--- | --- | --- | ---
Refrigerant | Type |  | HFC-134a (R-134a)
Capacity of system |  | 450−500 g (15.9−17.6 oz)
Refrigerant oil | Type |  | DENSO ND-OIL 8 (P/N 38897-PR7-003, 38898-PR7-003 or 38899-PR7-A01)
Capacity of components | Condenser | 25 mL (5/6 fl·oz, 0.9 Imp·oz)
Evaporator | 45 mL (1 1/2 fl·oz, 1.6 Imp·oz)
Each line and hose | 10 mL (1/3 fl·oz, 0.4 Imp·oz)
Compressor | 160−175 mL (5 1/3−5 2/3 fl·oz, 5.6−6.2 Imp·oz)
Compressor | Field coil resistance | At 20 °C (68 °F) | 3.9−4.3 Ω
Pulley-to-pressure plate clearance |  | 0.35−0.60 mm (0.014−0.024 in.)