DTC Troubleshooting: 8

DTC 8: A Short in the Evaporator Temperature Sensor Circuit Remove the evaporator temperature sensor. Test the evaporator temperature sensor. Is the resistance within the specifications shown on the graph?
YES | - | Go to Step 3 .
NO | - | Replace the evaporator temperature sensor .■
Disconnect audio-HVAC module 22P connector. Check for continuity between the No. 10 terminal of the audio-HVAC module 22P connector and body ground. Is there continuity?
YES | - | Repair short to body ground in the wire between the audio-HVAC module and the evaporator temperature sensor.■
NO | - | Substitute a known-good audio-HVAC module, and recheck. If the symptom/indication goes away, replace the original audio-HVAC module.■