Connect the No. 1 terminals of the magnet valve 2P connector to body ground with a jumper wire with the magnet valve connector connected. Turn the ignition switch ON (II). Does the magnet valve operate?
YES | - | Go to Step 9 .
NO | - | Replace the magnet valve, and recheck.■
Turn the ignition switch OFF, and disconnect the jumper wire. Disconnect the magnet valve 2P connector. Disconnect climate control unit connector B (16P). |