DTC P2017: IMRC Valve Position Sensor Circuit High Voltage Turn the ignition switch ON (II). Check the IMRC VALVE POSITION SENSOR in the DATA LIST with the HDS. Is about 4.90 V or higher indicated?
YES | - | Go to Step 3 .
NO | - | Intermittent failure, system is OK at this time. Check for poor connections or loose terminals at the IMRC valve position sensor and the ECM.■
Turn the ignition switch OFF. Disconnect the IMRC valve position sensor 3P connector. Connect IMRC valve position sensor 3P connector terminals No. 2 and No. 3 with a jumper wire. Turn the ignition switch ON (II). Check the IMRC VALVE POSITION SENSOR in the DATA LIST with the HDS. Is about 4.90 V or higher indicated?
YES | - | Go to Step 8 .
NO | - | Go to Step 19 .