Apply liquid gasket, P/N 08C70-K0234M or 08C70-K0334M, evenly to the block mating surface of the chain case. Apply liquid gasket to the block upper surface contact areas (A) and lower block upper surface contact areas (B) on the chain case. Apply liquid gasket, P/N 08C70-K0234M or 08C70-K0334M, evenly to the oil pan mating surface of the chain case. NOTE: Do not install the parts if 4 minutes or more have elapsed since applying liquid gasket. Instead, reapply liquid gasket after removing old residue. |