Fuse to Components Index - Under-hood Fuse/Relay Box

Under-hood Fuse/Relay Box

Fuse Number | Amps | Wire Color | Component(s) or Circuit(s) Protected
--- | --- | --- | ---
1 | 15 A | RED/YEL | Left headlight (low beam)
2 | 30 A | ——— | Control block
3 | 10 A | WHT/YEL | Left headlight (high beam)
4 | 15 A | ——— | Control block
RED/BLK | Parking lights, Taillights, License plate lights, A/T gear position console light, Ashtray light, Audio-AVAC-display module, Cigarette lighter light, Glove box light, Hazard warning switch light, Headlight adjuster switch light, Rear individual map lights, Sunroof switch light, TCS off switch light, VSA OFF switch
5 | 15 A | WHT/GRN | Right headlight (high beam)
6 | 15 A | RED/GRN | Right headlight (low beam)
7 | 7.5 A | ——— | Control block
8 | 15 A | WHT/GRN | PGM-FI main relay, Data link connector (DLC)
9 | 20 A | BLU/YEL | A/C condenser fan motor
10 | 20 A | YEL | Front fog lights (via front fog light relay), Front fog light relay
11 | 20 A | BLU/BLK | Radiator fan motor
12 | 30 A | BLU/RED | A/C compressor clutch
13 | 20 A | RED | ABS modulator-control unit, VSA modulator-control unit, Brake lights, ECM/PCM, Horns, Ignition key light
——— | Control block
14 | 40 A | BLK/YEL | Rear window defogger, Antenna amplifier
15 | 40 A | YEL | No. 7 fuse (in the under-hood fuse/relay box), No. 5, 6, 7, 8 and 9 fuses (in the under-hood fuse/relay box)
16 | 15 A | WHT/BLK | Turn signal/hazard relay (via hazard warning switch), Hazard warning light relay
17 | 30 A | WHT/RED | ABS modulator-control unit (MR +B), VSA modulator-control unit (MR +B)
18 | 40 A (with VSA) | WHT | ABS modulator-control unit (+B FSR), VSA modulator-control unit (+B FSR)
20 A (with ABS)
19 | 40 A | GRN/WHT | No. 1, 2, 3 and 4 fuses (in the under -dash fuse/relay box)
20 | 40 A | BLU | No. 12, 13, 14, 15, 16 and 17 fuses (in the under-dash fuse/relay box)
21 | 40 A | WHT/BLU | Blower motor
22 (BAT) | 100 A | ——— | Battery, Power distribution
22 (EPS) | 70 A | WHT | EPS control unit (+B)
23 (IG) | 50 A | WHT | Ignition switch, No. 12 fuse (in the under-dash fuse/relay box)
23 (P/W) | 40 A | WHT/BLU | Power window relay, No. 27, 28 fuses (in the under-dash fuse/relay box)