Inside Rearview Mirror Replacement - With Automatic Dimming

Disconnect the connector (A). Slide the mirror harness upper cover (B) forward, then remove the mirror harness cover (C) from the mirror base (D). |

Using a T20 Torx bit, loosen the screw, then slide the rearview mirror (A) rearward and off the mount (B). Install the mirror in the reverse order of removal, and note these items: Before installing the mirror, remove the Torx screw, and apply liquid thread lock to it. Make sure the connector is plugged in properly. |