1. Inspect the brake hoses for damage, deterioration, leaks, interference, and twisting. Check the brake lines for damage, rusting, and leaks. Also check for bent brake lines. Check for leaks at hose and line joints and connections, and retighten if necessary. Check the master cylinder and ABS or VSA modulator-control unit for damage and leaks. NOTE: Replace the brake hose clip whenever the brake hose is serviced.
   Connection Point | Component | Connected to | Specified Torque Value | Note
   --- | --- | --- | --- | ---
   A | Front brake caliper | Brake hose | 34 N·m (3.5 kgf·m, 25 lbf·ft) | Banjo bolt
   Bleed screw (Except NISSIN) | 9.8 N·m (1.0 kgf·m, 7.2 lbf·ft) |
   Bleed screw (NISSIN) | 9 N·m (0.9 kgf·m, 7 lbf·ft) |
   B | Rear brake caliper | Brake hose | 34 N·m (3.5 kgf·m, 25 lbf·ft) | Banjo bolt
   Bleed screw (Except NISSIN) | 9.8 N·m (1.0 kgf·m, 7.2 lbf·ft) |
   Bleed screw (NISSIN) | 9 N·m (0.9 kgf·m, 7 lbf·ft) |
   C | Brake hose | Brake line | 15 N·m (1.5 kgf·m, 11 lbf·ft) | Flare nut
   D | Master cylinder | Brake line (ABS) | 15 N·m (1.5 kgf·m, 11 lbf·ft) | Flare nut
   Brake line (VSA) | 29 N·m (3.0 kgf·m, 22 lbf·ft) | Flare nut
   E | ABS modulator-control unit | Brake line | 15 N·m (1.5 kgf·m, 11 lbf·ft) | Flare nut
   VSA modulator-control unit | Brake line (10 mm nut) | 15 N·m (1.5 kgf·m, 11 lbf·ft) | Flare nut
   Brake line (14 mm nut) | 29 N·m (3.0 kgf·m, 22 lbf·ft) | Flare nut
   F | Pressure sensor (ACC) | Brake line | 15 N·m (1.5 kgf·m, 11 lbf·ft) | Flare nut