CMP Pulse Plate Replacement

Remove the camshaft position (CMP) sensor. Remove the cylinder head cover. Hold the intake camshaft with an open-end wrench, then loosen the CMP pulse plate mounting bolt. |

1. Remove the CMP pulse plate. Install the CMP pulse plate and bolt. Hold the intake camshaft with an open -end wrench, then tighten the bolt.
   Specified Torque: | 12 N·m (1.2 kgf·m, 8.7 lbf·ft)
Install the cylinder head cover. Install the CMP sensor. |