Check for continuity between the terminals in each switch position according to the table. If the continuity checks do not agree with the table, replace the steering lock. After reconnecting the battery, enter the anti-theft code for the radio and the navigation system, then enter the customer's radio station presets. Do the engine idle learn procedure and the power window control unit reset procedure. |