Maintenance Schedule for Normal Conditions - Australia and New Zealand Models

Follow the Normal Conditions Maintenance Schedule if the severe driving conditions specified in the Severe Conditions Maintenance Schedule do not apply.

Service at the indicated distance or time whichever comes first | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
miles x 1,000 | 12.5 | 25.0 | 37.5 | 50.0 | 62.5 | 75.0 | 87.5 | 100.0 | 112.5 | 125.0
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
Replace engine oil | Every 10,000 km (6,250 miles) or 1 year
Replace engine oil filter | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●
Replace air cleaner element |  | ● |  | ● |  | ● |  | ● |  | ●
Inspect the valve clearance Check valve clearance |  | ● |  | ● |  | ● |  | ● |  | ●
Replace fuel filter |  |  |  | ● |  |  |  | ● |  |
Replace spark plugs |  |  |  |  | ● |  |  |  |  | ●
Inspect drive belt Check for cracks, damage, deflection, and tension |  | ● |  | ● |  | ● |  | ● |  | ●
Inspect idle speed |  |  |  |  | ● |  |  |  |  | ●
Replace engine coolant Use genuine Honda All Season Antifreeze/Coolant Type 2 | At 200,000 km (120,000 miles) or 10 years, then every 100,000 km (60,000 miles) or 5 years
Replace manual transmission fluid Use Honda MTF |  |  |  |  |  | ● |  |  |  |
Replace automatic transmission fluid Use Honda ATF-Z1 | At 120,000 km (75,000 miles) or 6 years, then every 80,000 km (50,000 miles) or 4 years
Inspect front and rear brakes Check the brake pad and disc thickness. Check for damage or cracks front pad , front disc , rear pad , rear disc Check the calipers for damage, leaks, and tightness | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●
Replace brake fluid Use only DOT 3 or DOT 4 brake fluid. We recommend genuine Honda Brake Fluid Check that brake fluid level is between upper and lower marks on the reservoir | Every 3 years
Check parking brake adjustment Check the parking brake operation | ● | ● |  | ● |  | ● |  | ● |  | ●
Replace dust and pollen filter | Every 30,000 km (18,750 miles) or 1 year
Check lights alignment Check the position of the headlights | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●
Test drive Check for road stability, noise, vibrations, and dashboard operation | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●
Rotate tyres Check tyre inflation and condition at least once one month | Every 10,000 km (6,250 miles)

Service at the indicated distance or time whichever comes first | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
miles x 1,000 | 12.5 | 25.0 | 37.5 | 50.0 | 62.5 | 75.0 | 87.5 | 100.0 | 112.5 | 125.0
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
Visually inspect the following items: Check for correct installation and position, check for cracks, deterioration, rust, and leaks Check tightness of screws, nuts, and joints. If necessary, retighten
Tie-rod ends, steering gearbox, and boots Check rack grease and steering linkage. Check the boot for damage and leaking grease | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●
Suspension components Check the bolts for tightness Check all dust cover for deterioration and damage
Driveshaft boots Check the boot and boot band for cracks Check rack grease
Brake hoses and lines (including VSA) Check the master cylinder and VSA modulator-control unit and leakage
All fluid levels and condition of fluids Check levels and check for leaks. If necessary, add engine coolant , MTF, ATF, brake fluid, windshield fluid
Exhaust system Check the exhaust pipe and muffler for damage, leaks, and tightness
Fuel lines and connections Check fuel lines for loose connections, cracks, and deterioration. Retighten loose connections and replace any damaged parts