Special Tools Required Driver 07749-0010000 Attachment, 78 x 80 mm 07NAD-PX40100 Preload inspection tool 07YAJ-S3V0100 If any of the items listed below were replaced, the carrier bearing preload must be adjusted. Transmission housing Clutch housing Differential carrier Spacer Carrier bearing and outer race Remove the oil seals from the transmission housing and clutch housing. If you replaced the carrier bearing on the transmission housing side of the carrier, remove and discard the bearing outer race. Heat up the transmission housing to about 100 °C (212 °F) with a heat gun (A), then remove the bearing outer race (B), spacer (C), and 81 mm shim (D). Do not heat the housing in excess of 100 °C (212 °F). |