Sunroof Limit Switch Adjustment

Remove the headliner. With the sunroof wrench, close the glass (A) fully: Make sure both link lifters (B) are parallel, and in the position shown. Check the glass fit to the roof panel and the glass height. With an open-end wrench, loosen the limit switch mounting bolts (C). Adjust the limit switch (D): Move the switch plate (E) a little at a time, then secure it at the position where you hear a faint click when the switch cam (F) pushes the limit switch (open/close). Check that the switch plate contacts the switch bracket (G). Check the operation of the glass (from the tilt-up position to fully closed position, from the fully open position to the fully closed position) by operating the sunroof switch. Adjust the switch plate until the glass open, and closes correctly. Reinstall all remaining parts in the reverse order of removal. |