Maintenance Schedule for Severe Conditions
140,000km(7year)

Follow the Severe Conditions Maintenance Schedule if the customer's vehicle is driven MAINLY under one or more of the following conditions:

- Driving less than 8 km (5 miles) per trip or, in freezing temperatures, driving less than 16 km (10 miles) per trip.
- Driving in extremely hot over 35 °C (95 °F) conditions.
- Extensive idling, or long periods of stop-and-go driving.
- Trailer towing, driving with a car-top carrier, or driving in mountainous conditions.
- Driving on muddy, dusty, or de-iced roads.

NOTE: If the customer's vehicle is driven OCCASIONALLY under severe conditions, follow the Normal Conditions Maintenance Schedule.

Service at the indicated distance or time whichever comes first

| Drain fuel filter

| Check parking brake adjustment
Check the parking brake operation

| Replace dust and pollen filter
When the customer drives primarily in urban areas that have high concentrations of soot in the air, under dusty conditions, or the air flow from the heating and cooling system becomes less than normal.

| Check lights alignment

| Test drive (noise, stability, dashboard operation)

| Check expirty date for IMS bottle (if equipped)

Visually inspect the following items:
|  | Check for correct installation and position, check for cracks, deterioration, rust, and leaks
|  | Check tightness of screws, nuts, and joints. If necessary, retighten

| Brake hoses and lines (including VSA)
Check the master cylinder and VSA modulator control-unit and leakage

| All fluid levels and condition of fluids
Check levels and check for leaks. If necessary, add engine coolant, MTF, brake fluid, power steering fluid , and windshield fluid

| Exhaust system
Check the catalytic converter heat shield, exhaust pipe, and muffler for damage, leaks, and tightness

| Fuel lines and connections
Check fuel lines for loose connections, cracks, and deterioration. Retighten loose connections and replace any damaged parts

| Tyre condition

Every 10,000 km (6,250 miles) or 6 months

| Replace engine oil

| Replace engine oil filter

| Inspect front and rear brakes
|  | Check the brake pad and disc thickness. Check for damage or cracks front pad, front disc, rear pad, rear disc
|  | Check the brake linings for cracking, grazing, wear, and contamination
|  | Check the calipers for damage, leaks, and tightness

Visually inspect the following items:

| Tie-rod ends, steering gearbox, and boots
Check rack grease and steering linkage. Check the boot for damage and leaking grease

| Suspension components
|  | Check the bolts for tightness
|  | Check all dust cover for deterioration and damage

| Driveshaft boots
|  | Check the boot and boot band for cracks
|  | Check rack grease

Every 20,000 km (12,500 miles)

| Replace air cleaner element
Use normal conditions except in dusty conditions

Every 60,000 km (37,500 miles) or 4 years

| Replace manual transmission fluid (MTF)
Use genuine Honda MTF

Every 3 years

| Replace brake fluid
|  | Use only DOT 3 or DOT 4 brake fluid. We recommend genuine Honda Brake Fluid
|  | Check that brake fluid level between the upper and lower marks on the reservoir

Every year

| Inspect vehicle corrosion:
refer to the Body Repair Manual
|  | External Paintwork and panel Corrosion Check
|  | Under body Corrosion Check