1. Warm up the engine to normal operating temperature (the radiator fan comes on). Apply the parking brake, and block both rear wheels. Start the engine, then shift to the D position while pressing the brake pedal. Press the accelerator pedal, and release it suddenly. The engine should not stall. Repeat step 2 in the D3 position. Connect the HDS to the DLC (A), and go to the A/T data list. NOTE: The illustration shows LHD model; RHD model is symmetrical. Test-drive the vehicle on a flat road in the D position. Check for abnormal noise and clutch slippage. While driving, check that the shift points occur at the proper speeds by monitoring the throttle position sensor voltage with the HDS and comparing your shift point speeds and voltage to those in the table. (The throttle position sensor voltage represents the throttle opening.) K20A6 Engine model: Upshift: D Position
   Throttle position sensor voltage: 0.8 V
   1st→2nd | 14−19 km/h (9−12 mph)
   2nd→3rd | 32−37 km/h (20−23 mph)
   3rd→4th | 47−53 km/h (29−33 mph)
   4th→5th | 63−71 km/h (39−44 mph)
   Lock-up ON | 77−89 km/h (48−55 mph)
   Throttle position sensor voltage: 2.25 V
   1st→2nd | 32−39 km/h (20−24 mph)
   2nd→3rd | 60−68 km/h (37−42 mph)
   3rd→4th | 93−103 km/h (58−64 mph)
   4th→5th | 166−182 km/h (103−113 mph)
   Lock-up ON | 174−192 km/h (108−119 mph)
   Fully-opened throttle Throttle position sensor voltage: 4.5 V
   1st→2nd | 55−63 km/h (34−39 mph)
   2nd→3rd | 103−116 km/h (64−72 mph)
   3rd→4th | 161−179 km/h (100−111 mph)
   4th→5th | ———
   Lock-up ON | ———
   K20A6 Engine model: Downshift: D Position
   Throttle position sensor voltage: 0.8 V
   Lock-up OFF | 76−85 km/h (47−53 mph)
   5th→4th | 48−56 km/h (30−35 mph)
   4th→3rd | 31−35 km/h (19−22 mph)
   3rd→1st | 8−13 km/h (5−8 mph)
   Throttle position sensor voltage: 2.25 V
   Lock-up OFF | 106−121 km/h (66−75 mph)
   Fully-opened throttle Throttle position sensor voltage: 4.5 V
   Lock-up OFF | 174−190 km/h (108−118 mph)
   5th→4th | 187−206 km/h (116−128 mph)
   4th→3rd | 137−153 km/h (85−95 mph)
   3rd→2nd | 87−98 km/h (54−61 mph)
   2nd→1st | 42−50 km/h (26−31 mph)
   K24A3 Engine model: Upshift: D Position
   Throttle position sensor voltage: 0.8 V
   1st→2nd | 14−19 km/h (9−12 mph)
   2nd→3rd | 32−37 km/h (20−23 mph)
   3rd→4th | 47−53 km/h (29−33 mph)
   4th→5th | 63−71 km/h (39−44 mph)
   Lock-up ON | 77−89 km/h (48−55 mph)
   Throttle position sensor voltage: 2.25 V
   1st→2nd | 32−39 km/h (20−24 mph)
   2nd→3rd | 60−68 km/h (37−42 mph)
   3rd→4th | 93−103 km/h (58−64 mph)
   4th→5th | 166−182 km/h (103−113 mph)
   Lock-up ON | 174−192 km/h (108−119 mph)
   Fully-opened throttle Throttle position sensor voltage: 4.5 V
   1st→2nd | 55−63 km/h (34−39 mph)
   2nd→3rd | 103−116 km/h (64−72 mph)
   3rd→4th | 161−179 km/h (100−111 mph)
   4th→5th | ———
   Lock-up ON | ———
   K24A3 Engine model: Downshift: D Position
   Throttle position sensor voltage: 0.8 V
   Lock-up OFF | 76−85 km/h (47−53 mph)
   5th→4th | 48−56 km/h (30−35 mph)
   4th→3rd | 31−35 km/h (19−22 mph)
   3rd→1st | 8−13 km/h (5−8 mph)
   Throttle position sensor voltage: 2.25 V
   Lock-up OFF | 106−121 km/h (66−75 mph)
   Fully-opened throttle Throttle position sensor voltage: 4.5 V
   Lock-up OFF | 174−190 km/h (108−118 mph)
   5th→4th | 187−206 km/h (116−128 mph)
   4th→3rd | 137−153 km/h (85−95 mph)
   3rd→2nd | 87−98 km/h (54−61 mph)
   2nd→1st | 42−50 km/h (26−31 mph)
Accelerate to about 57 km/h (35 mph) so the transmission is in 4th or 5th gear in M position, then shift to 2nd gear. The vehicle should immediately begin to slow down from engine braking. Check for abnormal noise and clutch slippage in the R position. Accelerate from a stop at full throttle, and check for abnormal noise and clutch slippage. Test in P (Park) Position.Park the vehicle on a slope (about 16 °), apply the brake, and shift into the P position. Release the brake; the vehicle should not move. NOTE: Always use the brake to hold the vehicle, when stopped on an incline in gear. Depending on the grade of the incline, the vehicle could roll backwards if the brake is released. |