ECM/PCM Idle Learn Procedure

The idle learn procedure must be done so the ECM/PCM can learn the engine idle characteristics. Do the idle learn procedure whenever you do any of these actions: The ECM/PCM is replaced. The ECM/PCM is reset. NOTE: Erasing DTCs with the HDS does not require you to do the idle learn procedure. The throttle body is replaced. The throttle body is cleaned. Procedure Make sure all electrical items (A/C, audio, rear window defogger, lights, etc.) are off. Reset the ECM/PCM with the HDS. Turn the ignition switch ON (II), and wait for 2 seconds. Start the engine. Hold the engine speed at 3,000 rpm (min −1 ) without load (in Park or neutral) until the radiator fan comes on, or until the engine coolant temperature reaches 90 °C (194 °F). Let the engine idle about 5 minutes with the throttle fully closed. NOTE: If the radiator fan comes on, do not include its running time in the 5 minutes. |