NOTE: Use fender covers to avoid damaging painted surfaces. Make sure you have the anti-theft codes for the radio and the navigation system, then write down the frequencies for the radio preset buttons. Disconnect the negative (−) cable first, then the positive (+) cable from the battery. Remove the battery. Remove the air cleaner housing. Remove the battery base (A), then remove the ground cable (B). Remove the intake air cover. |