1. DTC 11, 13, 15, 17: Wheel Sensor (Open/Short to Body Ground/Short to Power) Disconnect the VSA control unit 47P connector. Start the engine. Measure the voltage between body ground and the appropriate wheel sensor +B and GND terminals of the VSA control unit 47P connector individually (see table).
   DTC | Appropriate Terminal
   --- | ---
   +B | GND
   11 (Right-front) | FR +B: No. 34 | FR-GND: No. 33
   13 (Left-front) | FL +B: No. 45 | FL-GND: No. 46
   15 (Right-rear) | RR +B: No. 43 | RR-GND: No. 42
   17 (Left-rear) | RL +B: No. 36 | RL-GND: No. 37
Is there 1 V or more?
YES | - | Repair short to power in the wire between the VSA modulator-control unit and the appropriate wheel sensor.■
NO | - | Go to Step 4 .
Turn the ignition switch OFF. |