Intermediate Shaft Removal

Drain the transmission fluid. Reinstall the drain plug using a new washer. Remove the right driveshaft. Remove the exhaust pipe bracket. |

Remove the lower torque rod. |

Remove the flange bolt (A) and two dowel bolts (B). |

Remove the intermediate shaft (A) from the differential. Hold the intermediate shaft horizontal until it is clear of the differential to prevent damage to the differential oil seal (B). |