1. Remove the dipstick, and refill transmission with the recommended fluid amount through the opening of the dipstick guide pipe until the level reaches the upper mark on the dipstick. Always use genuine Honda ATF-Z1 automatic transmission fluid (ATF). Using a non-Honda ATF can affect shift quality.
   Automatic Transmission Fluid Capacity:
   2.9 L (3.1 US qt, 2.6 Imp qt) at change
   6.5 L (6.9 US qt, 5.7 Imp qt) at overhaul