1. In-vehicle Check that the seat belt is not twisted or caught on anything. After installing the anchors, check for free movement on the anchor bolts. If necessary, remove the anchor bolts and check that the washers and other parts are not damaged or improperly installed. Check the seat belts for damage or discoloration. Clean with a shop towel if necessary. Use only soap and water to clean. NOTE: Dirt buildup in the metal loops of the upper anchors can cause the seat belts to retract slowly. Wipe the inside of the loops with a clean cloth dampened in isopropyl alcohol. Check that the seat belt does not lock when pulled out slowly. The seat belt is designed to lock only during a sudden stop or impact. NOTE: The rear center seat belt which has been retracted does not lock because of the function of the seat belt lock canceller, refer to Step 5 . For rear center seat belt, check the seat belt lock canceller function. This function is working until the seat belt is pulled out from the retractor over the canceller off position: Check that the left seat-back does not be caught in the rear center seat belt when folding the seat-back forward speedily. Make sure that the seat belt will retract automatically when released. For rear passenger's seat belt, check the seat belt retractor locking mechanism ALR (automatic locking retractor). This function is for securing child seats.
   -1. | Pull the seat belt all the way out to engage the ALR. The seat belt should retract with a ratcheting sound, but not extend. This is normal.
   -2. | To disengage the ALR, release the seat belt and allow it to fully retract, then pull the seat belt out part-way. The seat belt should retract and extend normally.
Replace the seat belt with a new assembly if there is any abnormality. Do not disassemble any part of the seat belt for any reason. |