Use suction cups (A) to hold the quarter glass (B) over the opening, align the clips or the alignment marks (C) made in Step 12 , and set it down on the adhesive. Lightly push on the quarter glass until its edges are fully seated on the adhesive all the way around. Do not open or close the doors until the adhesive is dry. Scrape or wipe the excess adhesive off with a putty knife or towel. To remove adhesive from a painted surface or the quarter glass, wipe with a soft shop towel damaged with alcohol. Let the adhesive dry for at least 1 hour. |