Remove the heater hoses. Remove the intake manifold. Remove the exhaust manifold. Remove the exhaust gas recirculation (EGR) valve. Remove the fuel pump. Remove the engine wire harness connectors and wire harness clamps from the cylinder head. Four injector connectors Four glow plug connectors Engine coolant temperature (ECT) sensor connector Camshaft position (CMP) sensor connectors Turbocharger boost control solenoid connector Remove the cam chain. |