Front Fender Fairing Replacement

Remove the front inner fender as necessary. Open the front door. Remove the upper clip, and from inside the door, remove the lower clip securing the front fender fairing (A) and front fender (B). |

From the wheel arch, release the clips. |

Remove the front fender fairing (A). |

Install the fender fairing in the reverse order of removal, and note these items: Replace any damaged clips. Before installing the clips in the door opening area, install the front fender fairing (A) to the front fender (B) properly as shown. Push the clips into place securely. |