Clutch - 2/3

Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
Clutch - 2/3 | Clutch end plate-to-top-disc clearance (K24A3 engine) | 1st and 3rd | ——— | 0.82−1.02 mm (0.032−0.040 in.)
2nd | ——— | 0.88−1.08 mm (0.035−0.043 in.)
4th and 5th | ——— | 0.82−1.02 mm (0.032−0.040 in.)
Clutch return spring free length (K20A6 engine) | 1st, 2nd, and 3rd | 50.8 mm (2.00 in.) | 48.8 mm (1.92 in.)
4th and 5th | 33.5 mm (1.32 in.) | 31.5 mm (1.24 in.)
Clutch return spring free length (K24A3 engine) | 1st and 3rd | 38.0 mm (1.50 in.) | 36.0 mm (1.42 in.)
2nd | 50.8 mm (2.00 in.) | 48.8 mm (1.92 in.)
4th and 5th | 33.5 mm (1.32 in.) | 31.5 mm (1.24 in.)
Clutch disc thickness (K20A6 engine) | 1st, 2nd, 3rd, 4th, and 5th | 1.94 mm (0.076 in.) | ———
Clutch disc thickness (K24A3 engine) | 1st and 3rd | 1.96 mm (0.077 in.) | ———
2nd, 4th, and 5th | 1.94 mm (0.076 in.) | ———
Clutch plate thickness (K20A6 engine) | 1st, 2nd, 3rd, 4th, and 5th | 2.00 mm (0.079 in.) | When discolored
Clutch plate thickness (K24A3 engine) | 1st and 3rd | 1.6 mm (0.063 in.) | When discolored
2nd | 2.0 mm (0.079 in.) | When discolored
4.0 mm (0.157 in.) | When discolored
4th and 5th | 2.0 mm (0.079 in.) | When discolored
Clutch waved-plate phase difference |  | 0.07−0.20 mm (0.003−0.008 in.) | 0.05 mm (0.002 in.)
1st and 3rd clutch end plate thickness (K20A6 engine) | Mark 1 | 2.3 mm (0.090 in.) | When discolored
Mark 2 | 2.4 mm (0.094 in.) | When discolored
Mark 3 | 2.5 mm (0.098 in.) | When discolored
Mark 4 | 2.6 mm (0.102 in.) | When discolored
Mark 5 | 2.7 mm (0.106 in.) | When discolored
Mark 6 | 2.8 mm (0.110 in.) | When discolored
Mark 7 | 2.9 mm (0.114 in.) | When discolored
Mark 8 | 3.0 mm (0.118 in.) | When discolored
Mark 9 | 3.1 mm (0.122 in.) | When discolored
Mark 10 | 3.2 mm (0.126 in.) | When discolored
Mark 11 | 3.3 mm (0.130 in.) | When discolored
Mark 12 | 3.4 mm (0.134 in.) | When discolored
2nd clutch end plate thickness (K20A6 engine) | Mark 1 | 2.6 mm (0.102 in.) | When discolored
Mark 2 | 2.7 mm (0.106 in.) | When discolored
Mark 3 | 2.8 mm (0.110 in.) | When discolored
Mark 4 | 2.9 mm (0.114 in.) | When discolored
Mark 5 | 3.0 mm (0.118 in.) | When discolored
Mark 6 | 3.1 mm (0.122 in.) | When discolored
Mark 7 | 3.2 mm (0.126 in.) | When discolored
Mark 8 | 3.3 mm (0.130 in.) | When discolored
Mark 9 | 3.4 mm (0.134 in.) | When discolored
4th and 5th clutch end plate thickness (K20A6 engine) | Mark 11 | 3.0 mm (0.118 in.) | When discolored
Mark 12 | 3.1 mm (0.122 in.) | When discolored
Mark 13 | 3.2 mm (0.126 in.) | When discolored
Mark 14 | 3.3 mm (0.130 in.) | When discolored
Mark 15 | 3.4 mm (0.134 in.) | When discolored
Mark 16 | 3.5 mm (0.138 in.) | When discolored
Mark 17 | 3.6 mm (0.142 in.) | When discolored
Mark 18 | 3.7 mm (0.146 in.) | When discolored
Mark 19 | 3.8 mm (0.150 in.) | When discolored