1. Attach the fastener (A) with adhesive tape to the body. Be sure the fastener lines up with the alignment marks (B). If the old quarter glass is to be reinstalled (and either clip is broken off the molding), seal the body holes with pieces of urethane tape (C). Then set the quarter glass upright in the opening, and make alignment marks (D) across the quarter glass and body with a grease pencil at the four points shown. Be careful not to touch the quarter glass where adhesive will be applied.
   Fastener adhesive tape:
   | Thickness 0.6 mm (0.02 in.) Width 9.5 mm (0.37 in.)
Remove the quarter glass. |