1. Connect the starter to the battery as shown, and check that the motor turns and keeps rotating. If the electric current and motor speed meet the specifications when the battery voltage is at 11.5 V, the starter is working properly.
   Specifications |
   Electric Current: | 80 A or less
   Motor Speed: |
   1.6 kW model: | 2,300 rpm (min −1 ) or more
   1.2 kW model: | 2,600 rpm (min −1 ) or more