DENSO/MITSUBISHI Check the hold-in coil for continuity between the S terminal and the armature housing (ground). There should be continuity. If there is continuity, go to Step 2 . If there is no continuity, replace the solenoid. Check the pull-in coil for continuity between the S terminal and M terminal. There should be continuity. If there is continuity, the solenoid is OK. If there is no continuity, replace the solenoid. | DENSO: MITSUBISHI: