Maintenance Schedule for Normal Conditions
100,000miles(8year)

Follow the Normal Conditions Maintenance Schedule if the severe driving conditions specified in the Severe Conditions Maintenance Schedule do not apply.

Service at the indicated distance or time whichever comes first

| Replace engine oil

| Replace engine oil filter

| Inspect front and rear brakes
|  | Check the brake pad and disc thickness. Check for damage or cracks front pad , front disc , rear pad , rear disc
|  | Check the brake linings for cracking, grazing, wear, and contamination
|  | Check the calipers for damage, leaks, and tightness

| Check parking brake adjustment

| Check lights alignment
Check the position of the headlights

| Test drive
Check for road stability, noise, vibration, and dashboard operation

| Check expiry date for IMS bottle (if equipped)

| Inspect drive belts
Check for cracks, damage, deflection, and tension

Visually inspect the following items:
|  | Check for correct installation and position, check for cracks, deterioration, rust, and leaks
|  | Check tightness of screws, nuts, and joints. If necessary, retighten

| Tie-rod ends, steering gearbox, and boots
Check rack grease and steering linkage. Check the boot for damage and leaking grease

| Suspension components
|  | Check the bolts for tightness
|  | Check all dust cover for deterioration and damage

| Driveshaft boots
|  | Check the boot and boot band for cracks
|  | Check rack grease

| Brake hoses and lines (including ABS)
Check the master cylinder, proportioning control valve, and ABS modulator and leakage

| All fluid levels and condition of fluids
Check levels and check for leaks. If necessary, add engine coolant , MTF, ATF, brake fluid, power steering fluid, windshield fluid, and battery fluid

| Exhaust system
Check the exhaust pipe and muffler for damage, leaks, and tightness

| Fuel lines and connections
Check fuel lines for loose connections, cracks, and deterioration. Retighten loose connections and replace any damaged parts

| Tyre condition
Check for pressure, puncture, cuts, and irregular thread wear

Every 40,000 km (25,000 miles)

| Replace air cleaner element

| Replace spark plugs

| Inspect the valve clearance

Every 120,000 km (75,000 miles)

| Replace spark plugs

Every 30,000 km (18,750 miles) or 1 year

| Replace dust and pollen filter

Every 120,000 km (75,000 miles) or 8 years

| Replace manual transmission fluid (MTF)
Use Honda Manual Transmission Fluid MTF

At 120,000 km (75,000 miles) or 8 years, then every 80,000 km (50,000 miles) or 4 years

| Replace automatic transmission fluid (ATF)
Use Honda ATF-Z1

At 200,000 km (120,000 miles) or 10 years, then every 100,000 km (60,000 miles) or 5 years

| Replace engine coolant
Use genuine Honda All Season Antifreeze/Coolant Type 2

Every 3 years

| Replace brake fluid
Use only DOT 3 or DOT 4 brake fluid. We recommend genuine Honda Brake Fluid. Check that brake fluid level between the upper and lower marks on the reservoir